**NOTE:** Where a fire wall is necessary to separate buildings, each building is to be provided individual code criteria Tables 3 through 11. See IBC 503.1.2.

|  |  |
| --- | --- |
| **TABLE 3 BASIC BUILDING CODE INFORMATION** | |
| **CONSTRUCTION CLASSIFICATION** (IBC 602) | Type: |
| **OCCUPANCY CLASSIFICATION** (indicate all) (IBC 302 & 504.2) |  |
| **MOST RESTRICTIVE OCCUPANCY CLASSIFICATION** (IBC Tables 504.3, 504.4 & 506.2) |  |
| Mixed Occupancy (IBC 508) Yes  No | |
| Separated (IBC 506.2.2 & 508.4) Yes  No | |
| Non separated (IBC 508.3) Yes  No | |
| Does building require Incidental Use Area Separation? (IBC 509.1) Yes  No | |
| 2-way Communication Required (IBC 1009.6.5 & 1009.8) Yes  No | |
| Fire Apparatus Access and Water Line (IFC 503 & 507) Yes  No | |
| **OTHER FIRE PROTECTION SYSTEMS, DEVICES or FEATURES**  If the building has any special or notable fire protection or safety feature or hazard the designers should list them here, describe the performance characteristics and refer to locations in construction documents. (e.g. fire extinguishers, smoke- evacuation/control/compartments - IBC 414.1.3.) |  |