|  |
| --- |
| **TABLE 2 SOILS & SITE** |
| **SOILS INVESTIGATION** (If required) | Yes [ ]  No [ ]  per IBC 1803.2 |
| **SOILS CLASSIFICATION** |  |
| Site Class |        per IBC 1613.3.2 |
| Classes Soil of Materials (UCS System) |        per IBC 1803.5.1 |
| Allowable Footing Bearing Pressure |        psf |  |
| **MINIMUM DESIGN SOIL BEARING LOAD** |        psf |  per IBC table 1806.2 |
| **COMPACTION**  |  |  |
| Subgrade:       Percent |  | [ ] ASTM D698 [ ] ASTM D1557 [ ] AASHTO(only for paving & roads) |
| Base:       Percent |  | [ ] ASTM D698 [ ] ASTM D1557 [ ] AASHTO(only for paving & roads) |
| Other:       Percent |  | [ ] ASTM D698 [ ] ASTM D1557 [ ] AASHTO(only for paving & roads) |
| **MINIMUM DESIGN SOIL LATERAL LOAD**       psf per IBC 1610.1 |
| **FOOTINGS** |  |
| Undisturbed footingsCompacted Fill Material | Yes [ ]  No [ ] Yes [ ]  No [ ]  per IBC 1804.6 |
| **ELEVATIONS**  |  |
| Elevation of Water Table: |        MSL |
| Elevation of lowest footing: |        MSL |
| Elevation of lowest floor or basement: |        MSL |